{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":11,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C"]
[]
[]
[]
[]
["","","","","FHQ35CAVEB","FHQ50CAVEB","FHQ60CAVEB","FHQ71CAVEB","FHQ100CAVEB","FHQ125CAVEB","FHQ140CAVEB"]
["Schalldruckpegel","Heizen","Hoch","dB(A)","36","37","37","38","42","44","46"]
["","","Nom.","dB(A)","34","35","35","36","38","41","42"]
["","","Niedrig","dB(A)","31","32","33","34","34","37","38"]
["","Kühlung","Niedrig","dB(A)","31","32","33","34","34","37","38"]
["","","Hoch","dB(A)","36","37","37","38","42","44","46"]
["","","Nom.","dB(A)","34","35","35","36","38","41","42"]
["Standardzubehör","Installationsanleitung","","","Installationsanleitung","Installationsanleitung","Installationsanleitung","Installationsanleitung","Installationsanleitung","Installationsanleitung","Installationsanleitung"]
["","Bedienungsanleitung","","","Bedienungsanleitung","Bedienungsanleitung","Bedienungsanleitung","Bedienungsanleitung","Bedienungsanleitung","Bedienungsanleitung","Bedienungsanleitung"]
["","Konformitätserklärung","","","Konformitätserklärung","Konformitätserklärung","Konformitätserklärung","Konformitätserklärung","Konformitätserklärung","Konformitätserklärung","Konformitätserklärung"]
["","Kondensatschlauch","","","Kondensatschlauch","Kondensatschlauch","Kondensatschlauch","Kondensatschlauch","Kondensatschlauch","Kondensatschlauch","Kondensatschlauch"]
["","Klemmblech","","","Klemmblech","Klemmblech","Klemmblech","Klemmblech","Klemmblech","Klemmblech","Klemmblech"]
["","Unterlegscheibe für Aufhängung","","","Unterlegscheibe für Aufhängung","Unterlegscheibe für Aufhängung","Unterlegscheibe für Aufhängung","Unterlegscheibe für Aufhängung","Unterlegscheibe für Aufhängung","Unterlegscheibe für Aufhängung","Unterlegscheibe für Aufhängung"]
["","Klemmen","","","Klemmen","Klemmen","Klemmen","Klemmen","Klemmen","Klemmen","Klemmen"]
["","Installationsmuster","","","Installationsmuster","Installationsmuster","Installationsmuster","Installationsmuster","Installationsmuster","Installationsmuster","Installationsmuster"]
["","Verbindungsstückisolierung","","","Verbindungsstückisolierung","Verbindungsstückisolierung","Verbindungsstückisolierung","Verbindungsstückisolierung","Verbindungsstückisolierung","Verbindungsstückisolierung","Verbindungsstückisolierung"]
["","Dichtungsmaterial","","","Dichtungsmaterial","Dichtungsmaterial","Dichtungsmaterial","Dichtungsmaterial","Dichtungsmaterial","Dichtungsmaterial","Dichtungsmaterial"]
["","Kunststoffführung","","","Kunststoffführung","Kunststoffführung","Kunststoffführung","Kunststoffführung","Kunststoffführung","Kunststoffführung","Kunststoffführung"]
["","Verdrahtungsfixierung","","","Verdrahtungsfixierung","Verdrahtungsfixierung","Verdrahtungsfixierung","Verdrahtungsfixierung","Verdrahtungsfixierung","Verdrahtungsfixierung","Verdrahtungsfixierung"]
["","Schraube für Verdrahtungsfixierung","","","Schraube für Verdrahtungsfixierung","Schraube für Verdrahtungsfixierung","Schraube für Verdrahtungsfixierung","Schraube für Verdrahtungsfixierung","Schraube für Verdrahtungsfixierung","Schraube für Verdrahtungsfixierung","Schraube für Verdrahtungsfixierung"]
["Regelungssysteme","Wired remote control","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53"]
["Rohrleitungsanschlüsse","Flüssigkeit","AD","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Gas","AD","mm","9.5","12.7","12.7","15.9","15.9","15.9","15.9"]
["","Ableitung","","","VP20","VP20","VP20","VP20","VP20","VP20","VP20"]
["Sound power level","Kühlung","","dB(A)","53","54","54","55","60","62","64"]
["","Heizen","","dB(A)","53","54","54","55","60","62","64"]
["Abmessungen","Maßeinheit","Breite","mm","960","960","1,270","1,270","1,590","1,590","1,590"]
["","","Tiefe","mm","690","690","690","690","690","690","690"]
["","","Höhe","mm","235","235","235","235","235","235","235"]
["Gehäuse","Material","","","Kunststoff, Blech","Kunststoff, Blech","Kunststoff, Blech","Kunststoff, Blech","Kunststoff, Blech","Kunststoff, Blech","Kunststoff, Blech"]
["","Farbe","","","Reinweiß","Reinweiß","Reinweiß","Reinweiß","Reinweiß","Reinweiß","Reinweiß"]
["Gewicht","Maßeinheit","","kg","24","25","31","32","38","38","38"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frequenz","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Bezeichnung","","","VE","VE","VE","VE","VE","VE","VE"]
["","Spannung","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]