{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":5,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKEACB"]
[]
[]
[]
[]
["","","","","EKEACBVE"]
["Dimensions","Unité","Hauteur","mm","300"]
["","","Largeur","mm","400"]
["","","Profondeur","mm","150"]
["Poids","Unité","","kg","5.10"]
["Accessoires standard","Manuel d'installation et d'exploitation","","","1"]
["","Thermistance (R1T)","","","1"]
["","Thermistance (R2T)","","","1"]
["","Thermistance (R3T)","","","1"]
["","Thermistance (R4T)","","","1"]
["","Bande isolante 150x50","","","4"]
["","Mousse de caoutchouc CR","","","4"]
["","Supports de montage","","","4"]
["","Vis","","","4"]
["","Presse-étoupe pour cache-bornes M20","","","3"]
["","Écrou de blocage M20","","","3"]
["","Diamètre du joint torique : 20","","","3"]
["","Presse-étoupe pour cache-bornes M16","","","6"]
["","Écrou de blocage M16","","","6"]
["","Diamètre du joint torique : 16","","","6"]
["","Capuchon pour presse-étoupe de cache-bornes","","","3"]
["","Epissure fil à fil","","","8"]
["","Attache","","","8"]
["","Clé Fibox","","","1"]
["Power supply","Nom","","","VE"]
["","Phase","","","1~"]
["","Fréquence","","Hz","50/60"]
["","Tension","","V","220-240/220"]