{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":11,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C"]
[]
[]
[]
[]
["","","","","FHQ35CAVEB","FHQ50CAVEB","FHQ60CAVEB","FHQ71CAVEB","FHQ100CAVEB","FHQ125CAVEB","FHQ140CAVEB"]
["Niveau de pression sonore","Chauffage","Haut","dBA","36","37","37","38","42","44","46"]
["","","Nom.","dBA","34","35","35","36","38","41","42"]
["","","Bas","dBA","31","32","33","34","34","37","38"]
["","Rafraîchissement","Bas","dBA","31","32","33","34","34","37","38"]
["","","Haut","dBA","36","37","37","38","42","44","46"]
["","","Nom.","dBA","34","35","35","36","38","41","42"]
["Accessoires standard","Manuel d'installation","","","Manuel d'installation","Manuel d'installation","Manuel d'installation","Manuel d'installation","Manuel d'installation","Manuel d'installation","Manuel d'installation"]
["","Manuel d’utilisation","","","Manuel d’utilisation","Manuel d’utilisation","Manuel d’utilisation","Manuel d’utilisation","Manuel d’utilisation","Manuel d’utilisation","Manuel d’utilisation"]
["","Déclaration de conformité","","","Déclaration de conformité","Déclaration de conformité","Déclaration de conformité","Déclaration de conformité","Déclaration de conformité","Déclaration de conformité","Déclaration de conformité"]
["","Flexible d'évacuation","","","Flexible d'évacuation","Flexible d'évacuation","Flexible d'évacuation","Flexible d'évacuation","Flexible d'évacuation","Flexible d'évacuation","Flexible d'évacuation"]
["","Attache métallique","","","Attache métallique","Attache métallique","Attache métallique","Attache métallique","Attache métallique","Attache métallique","Attache métallique"]
["","Rondelle pour attache de suspension","","","Rondelle pour attache de suspension","Rondelle pour attache de suspension","Rondelle pour attache de suspension","Rondelle pour attache de suspension","Rondelle pour attache de suspension","Rondelle pour attache de suspension","Rondelle pour attache de suspension"]
["","Attaches","","","Attaches","Attaches","Attaches","Attaches","Attaches","Attaches","Attaches"]
["","Schéma d’installation","","","Schéma d’installation","Schéma d’installation","Schéma d’installation","Schéma d’installation","Schéma d’installation","Schéma d’installation","Schéma d’installation"]
["","Matériau isolant pour joints","","","Matériau isolant pour joints","Matériau isolant pour joints","Matériau isolant pour joints","Matériau isolant pour joints","Matériau isolant pour joints","Matériau isolant pour joints","Matériau isolant pour joints"]
["","Matériau d'étanchéité","","","Matériau d'étanchéité","Matériau d'étanchéité","Matériau d'étanchéité","Matériau d'étanchéité","Matériau d'étanchéité","Matériau d'étanchéité","Matériau d'étanchéité"]
["","Bague en résine","","","Bague en résine","Bague en résine","Bague en résine","Bague en résine","Bague en résine","Bague en résine","Bague en résine"]
["","Dispositif de fixation de câbles","","","Dispositif de fixation de câbles","Dispositif de fixation de câbles","Dispositif de fixation de câbles","Dispositif de fixation de câbles","Dispositif de fixation de câbles","Dispositif de fixation de câbles","Dispositif de fixation de câbles"]
["","Vis pour dispositif de fixation de câbles","","","Vis pour dispositif de fixation de câbles","Vis pour dispositif de fixation de câbles","Vis pour dispositif de fixation de câbles","Vis pour dispositif de fixation de câbles","Vis pour dispositif de fixation de câbles","Vis pour dispositif de fixation de câbles","Vis pour dispositif de fixation de câbles"]
["Systèmes de commande","Télécommande câblée","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53"]
["Piping connections","Liquide","DE","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Gaz","DE","mm","9.5","12.7","12.7","15.9","15.9","15.9","15.9"]
["","Drain","","","VP20","VP20","VP20","VP20","VP20","VP20","VP20"]
["Niveau de puissance sonore","Rafraîchissement","","dBA","53","54","54","55","60","62","64"]
["","Chauffage","","dBA","53","54","54","55","60","62","64"]
["Dimensions","Unité","Largeur","mm","960","960","1,270","1,270","1,590","1,590","1,590"]
["","","Profondeur","mm","690","690","690","690","690","690","690"]
["","","Hauteur","mm","235","235","235","235","235","235","235"]
["Caisson","Matériau","","","Résine, tôle","Résine, tôle","Résine, tôle","Résine, tôle","Résine, tôle","Résine, tôle","Résine, tôle"]
["","Colour","","","Blanc frais","Blanc frais","Blanc frais","Blanc frais","Blanc frais","Blanc frais","Blanc frais"]
["Poids","Unité","","kg","24","25","31","32","38","38","38"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~","1~"]
["","Fréquence","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Nom","","","VE","VE","VE","VE","VE","VE","VE"]
["","Tension","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]