{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2HND-A5A"]
[]
[]
[]
[]
["","","","","","D2HND012A5AA","D2HND018A5AA"]
["Gas","Consumi (G20)","","Min","m³/h","0.31","0.31"]
["","","","Max","m³/h","1.18","1.80"]
["","Consumi (G25)","","Min","m³/h","0.36","0.36"]
["","","","Max","m³/h","1.38","2.09"]
["","Consumi (G31)","","Min","m³/h","0.12","0.12"]
["","","","Max","m³/h","0.46","0.69"]
["","Classe NOx","","","","6","6"]
["","Livelli di NOx (G20)","","","mg/kWh","10","18"]
["Riscaldamento centralizzato","Assorbimento di calore Qn (valore calorifico netto)","Nom.","Min","kW","2.9","2.9"]
["","","","Max","kW","11.1","16.9"]
["","Assorbimento di calore Qn (valore calorifico lordo)","Nom.","Min","kW","3.2","3.2"]
["","","","Max","kW","12.3","18.8"]
["","Pn in uscita a 80/60°C","","Min","kW","2.8","2.8"]
["","","","Nom.","kW","10.8","16.4"]
["","Pn in uscita a 50/30°C","","Min","kW","3.1","3.1"]
["","","","Nom.","kW","12.0","18.0"]
["","Potenza a 37/30°C","","Nom.","kW","3.6","5.5"]
["","Temperatura acqua","","Max","°C","100","100"]
["Risc. amb.","Generale","","Classe efficienza stagionale riscaldamento ambienti","","A","A"]
["Aria di immissione","Concentrico","","","","Sì","Sì"]
["Gas combustibile","Temperatura","","Max","°C","60","68"]
["","Portata (G20)","","Max","kg/ora","18.4","28.0"]
["","Portata (G31)","","Max","kg/ora","17.2","26.0"]
["Rivestimento","Colore","","","","Bianco titanio (Ral9003)","Bianco titanio (Ral9003)"]
["","Materiale","","","","Lamiera d'acciaio zincata verniciata a polvere","Lamiera d'acciaio zincata verniciata a polvere"]
["Dimensioni","Unità","Altezza","Struttura","mm","590","590"]